(footprint "SolderJumperBridgedSmol"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Small SMD Solder Jumper, rounded pads, bridged")
	(tags "net tie solder jumper bridged")
	(property "Reference" "REF**"
		(at 0 -1.3 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "e5b1e289-9cf4-4ce7-9ea1-60e3ff9912ab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SolderJumper_2_Bridged"
		(at 0 1.9 180)
		(layer "F.Fab")
		(uuid "ed259e40-0090-464a-a577-86f9222b23d6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "58c802ad-922f-47cd-91fa-721a81deb2c1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a3ee7a62-18cb-4f14-88b6-a1282ce8bbdc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, closed/bridged"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "57f40dbd-e4cf-4b5a-a965-a5a9ef7c6239")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom)
	(net_tie_pad_groups "1, 2")
	(fp_poly
		(pts
			(xy -0.25 -0.2) (xy 0.25 -0.2) (xy 0.25 0.2) (xy -0.25 0.2)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.Cu")
		(uuid "fdb3c31b-6de2-4f67-b70d-7a52e727e355")
	)
	(fp_line
		(start -0.8 -0.5)
		(end -0.8 0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dbf0a62a-fe83-4df5-ad35-b58cf13a9305")
	)
	(fp_line
		(start -0.8 -0.5)
		(end 0.8 -0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6a0313ea-19d0-4ae3-a747-6adef8b68baf")
	)
	(fp_line
		(start 0.8 0.5)
		(end -0.8 0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "37a578b0-e683-4875-94e9-22b7725a2314")
	)
	(fp_line
		(start 0.8 0.5)
		(end 0.8 -0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5903375e-4867-4441-bdd4-9565b3e745a0")
	)
	(pad "1" smd roundrect
		(at -0.4 0)
		(size 0.5 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(zone_connect 2)
		(uuid "f34472b3-6e0d-4c05-b301-2fb1fdbb5a82")
	)
	(pad "2" smd roundrect
		(at 0.4 0 180)
		(size 0.5 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(zone_connect 2)
		(uuid "ceb05418-d9e1-4d74-8615-f340b62da4e9")
	)
)
