(footprint "SolderJumperSmol"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Small SMD Solder Jumper, rounded pads, open")
	(tags "solder jumper open")
	(property "Reference" "REF**"
		(at 0 -1.3 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "68527601-3eb7-4605-9c2c-0e490d4a3768")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SolderJumper_2_Open"
		(at 0 1.9 180)
		(layer "F.Fab")
		(uuid "36b3f2b6-2514-44eb-bcd1-7e24acb35ce6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3bb67709-ea0b-481b-9e9a-4305aa8228ce")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5b4f3e8a-28d3-4920-b0bd-aa98d44add11")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, open"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "22aa35c0-0213-46e8-9b6f-7837d321b7f1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -0.8 -0.5)
		(end -0.8 0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "acdfebc1-22da-4ab8-b8d4-0421032404b6")
	)
	(fp_line
		(start -0.8 -0.5)
		(end 0.8 -0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ac97b509-400c-4540-83ab-89770bcb0523")
	)
	(fp_line
		(start 0.8 0.5)
		(end -0.8 0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f7a90187-d0a0-4d51-af06-079e9ef32a06")
	)
	(fp_line
		(start 0.8 0.5)
		(end 0.8 -0.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b0669940-e802-4b51-ba16-d452e81d6e80")
	)
	(pad "1" smd roundrect
		(at -0.4 0)
		(size 0.5 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(zone_connect 2)
		(uuid "854756b8-fc00-4bd3-a00c-0a45b5382514")
	)
	(pad "2" smd roundrect
		(at 0.4 0 180)
		(size 0.5 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_right bottom_right)
		(zone_connect 2)
		(uuid "0302e24d-2a74-4082-ba1d-0ed5b2f59f29")
	)
)
